**SECTION 09 78 33 – INTERIOR WOOD PANELING**

1. **GENERAL**
   1. SUBMITTALS
      1. Action Submittals:
         1. Product Data: Manufacturer’s descriptive data and product attributes for wood materials.
         2. Samples: Verification samples.
   2. QUALITY ASSURANCE
      1. Installer Qualifications: Firm specializing in work of this Section, with minimum [2] [\_\_] years’ experience.
      2. Mockup: Minimum [\_\_ x \_\_] feet. Approved mockup [may] [may not] remain as part of the Work.
2. **PRODUCTS**
   1. MANUFACTURERS
      1. Contract Documents are based on products by ThermoryUSA, [www.thermoryusa.com](http://www.thermoryusa.com).
      2. Substitutions: [Refer to Division 01.] [Not permitted.]
   2. MATERIALS
      1. Interior Wood Paneling:
         1. Species: Thermo Aspen.
         2. Profile: STS4.
         3. Size: Nominally [1 x 4] [1 x 5] inches.
      2. Interior Wood Paneling:
         1. Species: Thermo Aspen.
         2. Profile: STEP.
         3. Size: Nominally 5/4 x 3 inches.
      3. Interior Wood Paneling:
         1. Species: Thermo Aspen.
         2. Profile: Kyte.
         3. Size: Nominally 1 x 4 inches.
      4. Interior Wood Paneling:
         1. Species: Thermo Aspen.
         2. Profile: Vire.
         3. Size: Nominally 1 x 4 inches.
      5. Interior Wood Paneling:
         1. Species: Thermo Aspen.
         2. Profile: SHP.
         3. Size: Nominally [1 x 4] [5/4 x 4] inches.
      6. Interior Wood Paneling:
         1. Species: Alder.
         2. Profile: STS4.
         3. Size: Nominally [1 x 4] [1 x 5] inches.
      7. Interior Wood Paneling:
         1. Species: Alder.
         2. Profile: STEP.
         3. Size: Nominally 5/4 x 3 inches.
      8. Interior Wood Paneling:
         1. Species: Alder.
         2. Profile: SHP.
         3. Size: Nominally [1 x 4] [5/4 x 4] inches.
      9. Interior Wood Paneling:
         1. Species: Thermo Magnolia.
         2. Profile: STS10.
         3. Size: Nominally 1 x 7 inches.
      10. Interior Wood Paneling:
          1. Species: Thermo Magnolia.
          2. Profile: SHP.
          3. Size: Nominally 1 5/4 x 4 inches.
      11. Interior Wood Paneling:
          1. Species: Thermo Spruce.
          2. Profile: STS4.
          3. Size: Nominally 1 x 4 inches.
      12. Interior Wood Paneling:
          1. Species: Thermo Spruce.
          2. Profile: SHP.
          3. Size: Nominally 5/4 x 4 inches.
   3. ACCESSORIES
      1. Fasteners: [Plain steel] [Hot-dip galvanized steel] [Stainless steel] [screws.] [nails.]
3. **EXECUTION**
   1. INSTALLATION
      1. Install in accordance with manufacturer's instructions.
      2. Fasten at maximum [12] [16] [\_\_] inches on center.

END OF SECTION